**ELECTRIC MOTOR EDUCATION**

**HOW TO USE THIS PUMP**

**MOST IMPORTANT:**

ONLY OPERATE IN A **CLOCKWISE** DIRECTION (Viewed on coupling)

ALWAYS DOUBLE CHECK THE CORRECT DIRECTION OF MOTOR ROTATION

**“PRIOR TO COUPLING THE MOTOR TO THE PUMP”**

ENSURE SUCTION HOSE IS **ALWAYS IMMERSED**.

BOTH BEFORE STARTING THE PUMP AND WHILE IN USE

 **WARNING**

**DO NOT LET THE PUMP RUN DRY**

Turn off **immediately** when container is drained

(pump becomes inoperable if run dry, and doing so voids warranty)

Not suitable for drinking water

Do not use with flammable or corrosive materials

**MAX. PMP RATINGS** (Water (H20))

RPM : 3000

Output : 50 lt/min (5/12 lt.s-1)(5/12 kg.s-1)

Pump height : 15m

Self-Priming : 3m

Outlet Pressure : 300 kp (kNm-2)